{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":2,"n_cols":1,"rows_kept":2,"flags":["formulas_cached_only"]}
["高压造影注射器管路系统技术要求"]
["1、全自动，无需护士服务机器，\n2、无需针筒，直接插造影剂和盐水瓶。             3、需有三个带有保护帽的穿刺针头、压力传感器、微粒过滤器、单向止回阀。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}